; Copyright (c) 2002 CodeMachine Incorporated. All Rights Reserved.
; Developed by CodeMachine Inc.(www.codemachine.com)

[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%SI%
DriverVer=23/07/2004,1.4.0.0

[SourceDisksNames]
1=%DISKID%,,,

[SourceDisksFiles]
UsbIo.sys = 1
Generic.sys = 1

[Manufacturer]
%MfgName%=Stollmann

[Stollmann]
%USB\VID_0742&PID_FF01.DeviceDesc%=USBIO.Dev, USB\VID_0742&PID_FF01

[DestinationDirs]
USBIO.Files.Ext = 10,System32\Drivers

[USBIO.Dev]
CopyFiles=USBIO.Files.Ext

[USBIO.Dev.NT]
CopyFiles=USBIO.Files.Ext

[USBIO.Dev.NT.Services]
Addservice = USBIO, 0x00000002, USBIO.AddService

[USBIO.AddService]
DisplayName    = %USBIO.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_AUTO_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\USBIO.sys
AddReg         = USBIO.AddReg
LoadOrderGroup = Base

[USBIO.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,USBIO.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2

[USBIO.Files.Ext]
UsbIO.sys
Generic.sys


;---------------------------------------------------------------;

[Strings]
SI="Stollmann"
MfgName="Stollmann"
DISKID="UsbIo Installation Disk"
USB\VID_0742&PID_FF01.DeviceDesc="Philips Smartcard Reader"
USBIO.SvcDesc="UsbIO.Sys (c) Stollmann TS, Austria"
